**Thermostatic Mixing valve INSTAmix®**

Thermostatic mixing valve for mixed water distribution.

Safety temperature lockable by the installer and no setting scale.

Scald protection: hot water supply cut totally and immediately if cold water supply is interrupted.

Temperature set secured by hexagonal socket screw (Allen key)

Protection against legionella.

Approved check-valves.

Limescale resistance.

Adjustable temperature from 30°C to 60°C.

Exceptional reliability.

Extra compact size.

Esthetic conception with nickel plated finish brass.

Can be installed in any position.

Nickel-plated finish (raw brass on request).

Approved ACS.